ReadMe for CanHomW datasets
Each file contains surface wind speed data series for one location, with the adjusted-to-station’s climate ID (AdjTo ClimID) and the data temporal resolution in the filename, e.g., AdjTo1018620_mly.txt and AdjTo1018620_dly.txt (mly stands for monthly, and dly for daily). 
1. Data unit and missing value code are given in the first line: 
#Data unit: km/h.  Missing value code: -99.90. 
2. Column titles (second line): 
#YEAR Month Day    OrgW      AhcQCdW Flag    HomW Flag    SourceClimID
The first three columns specify the dates. Monthly data have 00 in the Day column. 
The OrgW column is the original archived wind speeds.
The AhcQCdW column is the anemometer height change adjusted (if any) and quality-controlled (QCd) wind speeds. This data series was subjected to the homogenization procedures.
The HomW column is the homogenized wind speeds.
The SourceClimID column specifies the source station’s climate ID, i.e., the climate ID in which the original wind speeds are recorded and archived. One single SourceClimID in this column means that the data series contains no joining of stations.
3. Flags:
Ahc: the value was adjusted for a documented anemometer height change.
H (in the HomW column): the value was adjusted to homogenize the data series (i.e., to make it homogeneous with the adjusted-to-station data series).




     


